Scitech - EKIUM Stability Room and Chamber Mapping Readiness Checklist
Complete prior to study.
Use for scoping and pre‑study alignment (dimensions, setpoint/range, products/label claims, loads, door use, monitoring, power/alarms, safety/permits). 
Includes pre‑study tick‑boxes for drawings/HVAC/calibration/data integrity/challenges/approvals.
Site & Asset Details
[ ] Company:
[ ] Site / Address:
[ ] Contact name, role and mobile number:
[ ] Manufacturer/Model(s):
[ ] Approx. L x W x H (m) and volume (m3):
[ ] Setpoint and Tolerance (deg C):
[ ] Product types and label storage requirements:
[ ] Number of compressors/defrost function:
[ ] Current monitoring system (Manufacturer/model):
[ ] Empty/load patterns:
[ ] Backup power/UPS and alarm response:
Pre-study checks (tick or comment)
[ ] Current floor plan and/or racking layout available
[ ] Time synchronisation method confirmed
[ [ ] Door-opening and power-interruption tests agreed
Note: Acceptance criteria must align to product labels and risk assessment. This checklist does not replace a protocol.
